<!--
     The FreeBSD Documentation Project

     $FreeBSD$
-->

<chapter id="boot">
  <title>The FreeBSD Booting Process</title>

  <sect1 id="boot-synopsis">
    <title>Synopsis</title>
    <indexterm><primary>booting</primary></indexterm>
    <indexterm><primary>bootstrap</primary></indexterm>

    <para>The process of starting a computer and loading the operating system
      is referred to as <quote>the bootstrap process</quote>, or simply
      <quote>booting</quote>.  FreeBSD's boot process provides a great deal of
      flexibility in customizing what happens when you start the system,
      allowing you to select from different operating systems installed on the
      same computer, or even different versions of the same operating system
      or installed kernel.</para>

    <para>This chapter details the configuration options you can set and how
      to customize the FreeBSD boot process.  This includes everything that
      happens until the FreeBSD kernel has started, probed for devices, and
      started &man.init.8;.  If you are not quite sure when this happens, it
      occurs when the text color changes from bright white to grey.</para>

    <para>After reading this chapter, you will know:</para>

    <itemizedlist>
      <listitem>
	<para>What the components of the FreeBSD bootstrap system are, and how
	  they interact.</para>
      </listitem>

      <listitem>
	<para>The options you can give to the components in the FreeBSD
	  bootstrap to control the boot process.</para>
      </listitem>
      
      <listitem>
        <para>The basics of &man.device.hints.5;.</para>
      </listitem>
    </itemizedlist>

    <note>
      <title>x86 Only</title>

      <para>This chapter only describes the boot process for FreeBSD running
	on Intel x86 systems.</para>
    </note>
  </sect1>

  <sect1 id="boot-introduction">
    <title>The Booting Problem</title>

    <para>Turning on a computer and starting the operating system poses an
      interesting dilemma.  By definition, the computer does not know how to
      do anything until the operating system is started.  This includes
      running programs from the disk.  So if the computer can not run a
      program from the disk without the operating system, and the operating
      system programs are on the disk, how is the operating system
      started?</para>

    <para>This problem parallels one in the book <citetitle>The Adventures of
      Baron Munchausen</citetitle>.  A character had fallen part way down a
      manhole, and pulled himself out by grabbing his bootstraps, and
      lifting.  In the early days of computing the term
      <firstterm>bootstrap</firstterm> was applied to the mechanism used to
      load the operating system, which has become shortened to
      <quote>booting</quote>.</para>

    <para>On x86 hardware the Basic Input/Output System (BIOS) is responsible
      for loading the operating system.  To do this, the BIOS looks on the
      hard disk for the Master Boot Record (MBR), which must be located on a
      specific place on the disk.  The BIOS has enough knowledge to load and
      run the MBR, and assumes that the MBR can then carry out the rest of the
      tasks involved in loading the operating system.</para>

    <indexterm>
      <primary>BIOS</primary>
    </indexterm>

    <indexterm>
      <primary>Basic Input/Output System</primary>
      <see>BIOS</see>
    </indexterm>

    <para>If you only have one operating system installed on your disks then
      the standard MBR will suffice.  This MBR searches for the first bootable
      slice on the disk, and then runs the code on that slice to load the
      remainder of the operating system.</para>

    <para>If you have installed multiple operating systems on your disks then
      you can install a different MBR, one that can display a list of
      different operating systems, and allows you to choose the one to boot
      from.  FreeBSD comes with one such MBR which can be installed, and other
      operating system vendors also provide alternative MBRs.</para>

    <para>The remainder of the FreeBSD bootstrap system is divided into three
      stages.  The first stage is run by the MBR, which knows just enough to
      get the computer into a specific state and run the second stage.  The
      second stage can do a little bit more, before running the third stage.
      The third stage finishes the task of loading the operating system.  The
      work is split into these three stages because the PC standards put
      limits on the size of the programs that can be run at stages one and
      two.  Chaining the tasks together allows FreeBSD to provide a more
      flexible loader.</para>

    <indexterm><primary>kernel</primary></indexterm>
    <indexterm><primary><command>init</command></primary></indexterm>

    <para>The kernel is then started and it begins to probe for devices
      and initialize them for use.  Once the kernel boot
      process is finished, the kernel passes control to the user process
      &man.init.8;, which then makes sure the disks are in a usable state.
      &man.init.8; then starts the user-level resource configuration which
      mounts file systems, sets up network cards to communicate on the
      network, and generally starts all the processes that usually
      are run on a FreeBSD system at startup.</para>
  </sect1>

  <sect1 id="boot-blocks">
    <title>The MBR, and Boot Stages One, Two, and Three</title>

    <sect2 id="boot-boot0">
      <title>MBR, <filename>/boot/boot0</filename></title>
      <indexterm><primary>Master Boot Record (MBR)</primary></indexterm>

      <para>The FreeBSD MBR is located in <filename>/boot/boot0</filename>.
	This is a <emphasis>copy</emphasis> of the MBR, as the real MBR must
	be placed on a special part of the disk, outside the FreeBSD
	area.</para>

      <para><filename>boot0</filename> is very simple, since the
	program in the <abbrev>MBR</abbrev> can only be 512 bytes in
	size.  If you have installed the FreeBSD MBR and have installed
	multiple operating systems on your hard disks then you will see a
	display similar to this one at boot time:</para>

      <example id="boot-boot0-example">
	<title><filename>boot0</filename> Screenshot</title>

	<screen>F1 DOS
F2 FreeBSD
F3 Linux
F4 ??
F5 Drive 1

Default: F2</screen>
      </example>

      <para>Other operating systems, in particular &windows;, have been known
	to overwrite an existing MBR with their own.  If this happens to you,
	or you want to replace your existing MBR with the FreeBSD MBR then use
	the following command:</para>

      <screen>&prompt.root; <userinput>fdisk -B -b /boot/boot0 <replaceable>device</replaceable></userinput></screen>

      <para>Where <replaceable>device</replaceable> is the device that you
	boot from, such as <devicename>ad0</devicename> for the first IDE
	disk, <devicename>ad2</devicename> for the first IDE disk on a second
	IDE controller, <devicename>da0</devicename> for the first SCSI disk,
	and so on.</para>

      <para>If you are a Linux user, however, and prefer that
	<application>LILO</application> control the boot process, you can
	edit the <filename>/etc/lilo.conf</filename> file for FreeBSD, or
	select <option>Leave The Master Boot Record Untouched</option>
	during the FreeBSD installation process.  If you have installed the
	FreeBSD boot manager, you can boot back into Linux and modify the
	<application>LILO</application> configuration file
	<filename>/etc/lilo.conf</filename> and add the following
	option:</para>

      <programlisting>other=/dev/hdXY
table=/dev/hdb
loader=/boot/chain.b
label=FreeBSD</programlisting>

      <para>which will permit the booting of FreeBSD and Linux via
	<application>LILO</application>.  In our example, we use
	<replaceable>XY</replaceable> to determine drive number and
	partition.  If you are using a <acronym>SCSI</acronym> drive, you
	will want to change <replaceable>/dev/hdXY</replaceable> to read
	something similar to <replaceable>/dev/sdXY</replaceable>, which
	again uses the <replaceable>XY</replaceable> syntax.  The
	<option>loader=/boot/chain.b</option> can be omitted if you have
	both operating systems on the same drive.  You can now run
	<command>/sbin/lilo -v</command> to commit your new changes to the
	system, this should be verified with screen messages.</para>
    </sect2>
  
    <sect2 id="boot-boot1">
      <title>Stage One, <filename>/boot/boot1</filename>, and Stage Two,
	<filename>/boot/boot2</filename></title>
      
      <para>Conceptually the first and second stages are part of the same
	program, on the same area of the disk.  Because of space constraints
	they have been split into two, but you would always install them
	together.</para>

      <para>They are found on the boot sector of
	the boot slice, which is where <link
	  linkend="boot-boot0">boot0</link>, or any other program on the
	<abbrev>MBR</abbrev> expects to find the program to run to
	continue the boot process.  The files in the
	<filename>/boot</filename> directory are copies of the real files,
	which are stored outside of the FreeBSD file system.</para>

      <para><filename>boot1</filename> is very simple, since it too 
	can only be 512 bytes
	in size, and knows just enough about the FreeBSD
	<firstterm>disklabel</firstterm>, which stores information
	about the slice, to find and execute <filename>boot2</filename>.</para>
      
      <para><filename>boot2</filename> is slightly more sophisticated, and understands
	the FreeBSD file system enough to find files on it, and can
	provide a simple interface to choose the kernel or loader to
	run.</para>

      <para>Since the <link linkend="boot-loader">loader</link> is
	much more sophisticated, and provides a nice easy-to-use
	boot configuration, <filename>boot2</filename> usually runs
	it, but previously it
	was tasked to run the kernel directly.</para>

      <example id="boot-boot2-example">
	<title><filename>boot2</filename> Screenshot</title>

	<screen>&gt;&gt; FreeBSD/i386 BOOT
Default: 0:ad(0,a)/kernel
boot:</screen>
      </example>

      <para>If you ever need to replace the installed
	<filename>boot1</filename> and <filename>boot2</filename> use
	&man.disklabel.8;:</para>
      
      <screen>&prompt.root; <userinput>disklabel -B <replaceable>diskslice</replaceable></userinput></screen>

      <para>where <replaceable>diskslice</replaceable> is the disk and slice
	you boot from, such as <devicename>ad0s1</devicename> for the first
	slice on the first IDE disk.</para>

      <warning>
	<title>Dangerously Dedicated Mode</title>

	<para>If you use just the disk name, such as
	  <devicename>ad0</devicename>, in the &man.disklabel.8; command you
	  will create a dangerously dedicated disk, without slices.  This is
	  almost certainly not what you want to do, so make sure you double
	  check the &man.disklabel.8; command before you press
	  <keycap>Return</keycap>.</para>
      </warning>
    </sect2>

  <sect2 id="boot-loader">
    <title>Stage Three, <filename>/boot/loader</filename></title>

    <indexterm><primary>boot-loader</primary></indexterm>
    <para>The loader is the final stage of the three-stage
      bootstrap, and is located on the file system, usually as
      <filename>/boot/loader</filename>.</para>
      
    <para>The loader is intended as a user-friendly method for
      configuration, using an easy-to-use built-in command set,
      backed up by a more powerful interpreter, with a more complex
      command set.</para> 

    <sect3 id="boot-loader-flow">
      <title>Loader Program Flow</title>
      
      <para>During initialization, the loader will probe for a
	console and for disks, and figure out what disk it is
	booting from.  It will set variables accordingly, and an
	interpreter is started where user commands can be passed from
	a script or interactively.</para>
      <indexterm><primary>loader</primary></indexterm>
      <indexterm><primary>loader configuration</primary></indexterm>

      <para>The loader will then read
	<filename>/boot/loader.rc</filename>, which by default reads
	in <filename>/boot/defaults/loader.conf</filename> which
	sets reasonable defaults for variables and reads
	<filename>/boot/loader.conf</filename> for local changes to
	those variables.  <filename>loader.rc</filename> then acts
	on these variables, loading whichever modules and kernel are
	selected.</para>

      <para>Finally, by default, the loader issues a 10 second wait
	for key presses, and boots the kernel if it is not interrupted.
	If interrupted, the user is presented with a prompt which
	understands the easy-to-use command set, where the user may
	adjust variables, unload all modules, load modules, and then
	finally boot or reboot.</para>

    </sect3>
    
    <sect3 id="boot-loader-commands">
      <title>Loader Built-In Commands</title>
      
      <para>These are the most commonly used loader commands.  For a
        complete discussion of all available commands, please see
        &man.loader.8;.</para>

      <variablelist>
	<varlistentry>
	  <term>autoboot <replaceable>seconds</replaceable></term>

	  <listitem>
	    <para>Proceeds to boot the kernel if not interrupted
	      within the time span given, in seconds.  It displays a
	      countdown, and the default time span is 10
	      seconds.</para>
	  </listitem>
	</varlistentry>

	<varlistentry>
	  <term>boot
	    <optional><replaceable>-options</replaceable></optional>
	    <optional><replaceable>kernelname</replaceable></optional></term>

	  <listitem>
	    <para>Immediately proceeds to boot the kernel, with the
	      given options, if any, and with the kernel name given,
	      if it is.</para>
	  </listitem>
	</varlistentry>

	<varlistentry>
	  <term>boot-conf</term>

	  <listitem>
	    <para>Goes through the same automatic configuration of
	      modules based on variables as what happens at boot.
	      This only makes sense if you use
	      <command>unload</command> first, and change some
	      variables, most commonly <envar>kernel</envar>.</para>
	  </listitem>
	</varlistentry>

	<varlistentry>
	  <term>help
	    <optional><replaceable>topic</replaceable></optional></term>

	  <listitem>
	    <para>Shows help messages read from
	      <filename>/boot/loader.help</filename>.  If the topic
	      given is <literal>index</literal>, then the list of
	      available topics is given.</para>
	  </listitem>
	</varlistentry>

	<varlistentry>
	  <term>include <replaceable>filename</replaceable>
	    &hellip;</term>

	  <listitem>
	    <para>Processes the file with the given filename.  The
	      file is read in, and interpreted line by line.  An
	      error immediately stops the include command.</para>
	  </listitem>
	</varlistentry>
	<varlistentry>
	  <term>load <optional><option>-t</option>
	    <replaceable>type</replaceable></optional>
	    <replaceable>filename</replaceable></term>

	  <listitem>
	    <para>Loads the kernel, kernel module, or file of the
	      type given, with the filename given.  Any arguments
	      after filename are passed to the file.</para>
	  </listitem>
	</varlistentry>
	<varlistentry>
	  <term>ls <optional><option>-l</option></optional>
	    <optional><replaceable>path</replaceable></optional></term>

	  <listitem>
	    <para>Displays a listing of files in the given path, or
	      the root directory, if the path is not specified.  If
	      <option>-l</option> is specified, file sizes will be
	      shown too.</para>
	  </listitem>
	</varlistentry>
	<varlistentry>
	  <term>lsdev <optional><option>-v</option></optional></term>

	  <listitem>
	    <para>Lists all of the devices from which it may be
	      possible to load modules. If <option>-v</option> is
	      specified, more details are printed.</para>
	  </listitem>
	</varlistentry>

	<varlistentry>
	  <term>lsmod <optional><option>-v</option></optional></term>

	  <listitem>
	    <para>Displays loaded modules. If <option>-v</option> is
	      specified, more details are shown.</para>
	  </listitem>
	</varlistentry>

	<varlistentry>
	  <term>more <replaceable>filename</replaceable></term>

	  <listitem>
	    <para>Displays the files specified, with a pause at each
	      <varname>LINES</varname> displayed.</para>
	  </listitem>
	</varlistentry>

	<varlistentry>
	  <term>reboot</term>

	  <listitem>
	    <para>Immediately reboots the system.</para>
	  </listitem>
	</varlistentry>

	<varlistentry>
	  <term>set <replaceable>variable</replaceable></term>
	  <term>set
	    <replaceable>variable</replaceable>=<replaceable>value</replaceable></term>

	  <listitem>
	    <para>Sets the loader's environment variables.</para>
	  </listitem>
	</varlistentry>

	<varlistentry>
	  <term>unload</term>

	  <listitem>
	    <para>Removes all loaded modules.</para>
	  </listitem>
	</varlistentry>
      </variablelist>
    </sect3>

    <sect3 id="boot-loader-examples">
      <title>Loader Examples</title>

      <para>Here are some practical examples of loader usage:</para>

      <itemizedlist>
	<indexterm><primary>single-user mode</primary></indexterm>
	<listitem>
	  <para>To simply boot your usual kernel, but in single-user
	    mode:</para>

	  <screen><userinput>boot -s</userinput></screen>
	</listitem>

	<listitem>
	  <para>To unload your usual kernel and modules, and then
	    load just your old (or another) kernel:</para>
    <indexterm>
      <primary><filename>kernel.old</filename></primary>
    </indexterm>

	  <screen><userinput>unload</userinput>
<userinput>load <replaceable>kernel.old</replaceable></userinput></screen>

	  <para>You can use <filename>kernel.GENERIC</filename> to
	    refer to the generic kernel that comes on the install
	    disk, or <filename>kernel.old</filename> to refer to
	    your previously installed kernel (when you have upgraded
	    or configured your own kernel, for example).</para>

	  <note>
	    <para>Use the following to load your usual modules with
	      another kernel:</para>

	    <screen><userinput>unload</userinput>
<userinput>set kernel="<replaceable>kernel.old</replaceable>"</userinput>
<userinput>boot-conf</userinput></screen></note>
	</listitem>

	<listitem>
	  <para>To load a kernel configuration script (an automated
	    script which does the things you would normally do in the
	    kernel boot-time configurator):</para>

	  <screen><userinput>load -t userconfig_script <replaceable>/boot/kernel.conf</replaceable></userinput></screen>
	</listitem>
      </itemizedlist>
  </sect3>
    </sect2>
  </sect1>

  <sect1 id="boot-kernel">
    <title>Kernel Interaction During Boot</title>
    <indexterm>
      <primary>kernel</primary>
      <secondary>boot interaction</secondary>
    </indexterm>
    
    <para>Once the kernel is loaded by either <link
	linkend="boot-loader">loader</link> (as usual) or <link
	linkend="boot-boot1">boot2</link> (bypassing the loader), it
      examines its boot flags, if any, and adjusts its behavior as
      necessary.</para>

    <sect2 id="boot-kernel-bootflags">
      <indexterm>
        <primary>kernel</primary>
        <secondary>bootflags</secondary>
      </indexterm>
      <title>Kernel Boot Flags</title>

      <para>Here are the more common boot flags:</para>

      <variablelist id="boot-kernel-bootflags-list">
	<varlistentry>
	  <term><option>-a</option></term>

	  <listitem>
	    <para>during kernel initialization, ask for the device
	      to mount as the root file system.</para>
	  </listitem>
	</varlistentry>

	<varlistentry>
	  <term><option>-C</option></term>

	  <listitem>
	    <para>boot from CDROM.</para>
	  </listitem>
	</varlistentry>

	<varlistentry>
	  <term><option>-c</option></term>

	  <listitem>
	    <para>run UserConfig, the boot-time kernel
	      configurator</para>
	  </listitem>
	</varlistentry>

	<varlistentry>
	  <term><option>-s</option></term>

	  <listitem>
	    <para>boot into single-user mode</para>
	  </listitem>
	</varlistentry>

	<varlistentry>
	  <term><option>-v</option></term>

	  <listitem>
	    <para>be more verbose during kernel startup</para>
	  </listitem>
	</varlistentry>
      </variablelist>

      <note>
	<para>There are other boot flags, read &man.boot.8; for more
	  information on them.</para></note>
    </sect2>

<!--    <sect2 id="boot-kernel-userconfig">
      <title>UserConfig: the Boot-time Kernel Configurator</title>
      
      <para> </para>
    </sect2> -->
  </sect1>
  
  <sect1 id="device-hints">
    <sect1info>
      <authorgroup>
	<author>
	  <firstname>Tom</firstname>
	  <surname>Rhodes</surname>
	  <contrib>Contributed by </contrib>
	</author>
      </authorgroup>
      <!-- 18 OCT 2002 -->
    </sect1info>
    <indexterm>
      <primary>device.hints</primary>
    </indexterm>
    <title>Device Hints</title>

    <note><para>This is a FreeBSD&nbsp;5.0 and later feature which does not
      exist in earlier versions.</para></note>

    <para>During initial system startup, the boot &man.loader.8; will read the
      &man.device.hints.5; file.  This file stores kernel boot information
      known as variables, sometimes referred to as <quote>device hints</quote>.
      These <quote>device hints</quote> are used by device drivers for device
      configuration.</para>
      
    <para>Device hints may also be specified at the <link linkend="boot-loader">
      Stage 3 boot loader</link> prompt.  Variables can be added using
      <command>set</command>, removed with <command>unset</command>, and viewed
      with the <command>show</command> commands.  Variables set in the
      <filename>/boot/device.hints</filename> file can be overridden here also.  Device hints entered at
      the boot loader are not permanent and will be forgotten on the next
      reboot.</para>

    <para>Once the system is booted, the &man.kenv.1; command can be used to
      dump all of the variables.</para>

    <para>The syntax for the <filename>/boot/device.hints</filename> file is one variable per line, using
      the standard hash <quote>#</quote> as comment markers.  Lines are
      constructed as follows:</para>

    <screen><userinput>hint.driver.unit.keyword="<replaceable>value</replaceable>"</userinput></screen>

    <para>The syntax for the Stage 3 boot loader is:</para>
    <screen><userinput>set hint.driver.unit.keyword=<replaceable>value</replaceable></userinput></screen>

    <para><literal>driver</literal> is the device driver name, <literal>unit</literal>
      is the device driver unit number, and <literal>keyword</literal> is the hint
      keyword.  The keyword may consist of the following options:</para>

    <itemizedlist>
      <listitem>
	<para><literal>at</literal>: specifies the bus which the device is attached to.</para>
      </listitem>

      <listitem>
	<para><literal>port</literal>: specifies the start address of the <acronym>I/O</acronym>
	  to be used.</para>
      </listitem>

      <listitem>
	<para><literal>irq</literal>: specifies the interrupt request number to be used.</para>
      </listitem>

      <listitem>
	<para><literal>drq</literal>: specifies the DMA channel number.</para>
      </listitem>

      <listitem>
	<para><literal>maddr</literal>: specifies the physical memory address occupied by the
	  device.</para>
      </listitem>

      <listitem>
	<para><literal>flags</literal>: sets various flag bits for the device.</para>
      </listitem>

      <listitem>
	<para><literal>disabled</literal>: if set to <literal>1</literal> the device is disabled.</para>
      </listitem>
    </itemizedlist>

    <para>Device drivers may accept (or require) more hints not listed here, viewing
      their manual page is recommended.  For more information, consult the
      &man.device.hints.5;, &man.kenv.1;, &man.loader.conf.5;, and &man.loader.8;
      manual pages.</para>
  </sect1>

  <sect1 id="boot-init">
    <indexterm>
      <primary><command>init</command></primary>
    </indexterm>
    <title>Init: Process Control Initialization</title>
	
    <para>Once the kernel has finished booting, it passes control to
      the user process &man.init.8;, which is located at
      <filename>/sbin/init</filename>, or the program path specified
      in the <envar>init_path</envar> variable in
      <command>loader</command>.</para>

    <sect2 id="boot-autoreboot">
      <title>Automatic Reboot Sequence</title>
      
      <para>The automatic reboot sequence makes sure that the
	file systems available on the system are consistent.  If they
	are not, and &man.fsck.8; cannot fix the
	inconsistencies, &man.init.8; drops the system
	into <link linkend="boot-singleuser">single-user mode</link>
	for the system administrator to take care of the problems
	directly.</para>
    </sect2>

    <sect2 id="boot-singleuser">
      <title>Single-User Mode</title>
      <indexterm><primary>single-user mode</primary></indexterm>
      <indexterm><primary>console</primary></indexterm>
      
      <para>This mode can be reached through the <link
	  linkend="boot-autoreboot">automatic reboot
	  sequence</link>, or by the user booting with the
	<option>-s</option> option or setting the
	<envar>boot_single</envar> variable in
	<command>loader</command>.</para>

      <para>It can also be reached by calling
	&man.shutdown.8; without the reboot
	(<option>-r</option>) or halt (<option>-h</option>) options,
	from <link linkend="boot-multiuser">multi-user
	  mode</link>.</para>

      <para>If the system <literal>console</literal> is set
	to <literal>insecure</literal> in <filename>/etc/ttys</filename>,
	then the system prompts for the <username>root</username> password
	before initiating single-user mode.</para>

      <example id="boot-insecure-console">
	<title>An Insecure Console in <filename>/etc/ttys</filename></title>

	<programlisting># name  getty                           type    status          comments
#
# If console is marked "insecure", then init will ask for the root password
# when going to single-user mode.
console none                            unknown off insecure</programlisting>
      </example>

      <note>
	<para>An <literal>insecure</literal> console means that you
	  consider your physical security to the console to be
	  insecure, and want to make sure only someone who knows the
	  <username>root</username> password may use single-user mode, and it
	  does not mean that you want to run your console insecurely.  Thus,
	  if you want security, choose <literal>insecure</literal>,
	  not <literal>secure</literal>.</para>
      </note>
    </sect2>
    
    <sect2 id="boot-multiuser">
      <title>Multi-User Mode</title>
      <indexterm><primary>multi-user mode</primary></indexterm>
      
      <para>If &man.init.8; finds your file systems to be
	in order, or once the user has finished in <link
	  linkend="boot-singleuser">single-user mode</link>, the
	system enters multi-user mode, in which it starts the
	resource configuration of the system.</para>

      <sect3 id="boot-rc">
      <indexterm><primary>rc files</primary></indexterm>
	<title>Resource Configuration (rc)</title>

	<para>The resource configuration system reads in
	  configuration defaults from
	  <filename>/etc/defaults/rc.conf</filename>, and
	  system-specific details from
	  <filename>/etc/rc.conf</filename>, and then proceeds to
	  mount the system file systems mentioned in
	  <filename>/etc/fstab</filename>, start up networking
	  services, start up miscellaneous system daemons, and
	  finally runs the startup scripts of locally installed
	  packages.</para>

	<para>The &man.rc.8; manual page is a good reference to the resource
	  configuration system, as is examining the scripts
	  themselves.</para>
      </sect3>
    </sect2>
  </sect1>

  <sect1 id="boot-shutdown">
    <title>Shutdown Sequence</title>
    <indexterm>
      <primary><command>shutdown</command></primary>
    </indexterm>

    <para>Upon controlled shutdown, via &man.shutdown.8;,
      &man.init.8; will attempt to run the script
      <filename>/etc/rc.shutdown</filename>, and then proceed to send
      all processes the <literal>TERM</literal> signal, and subsequently 
      the <literal>KILL</literal> signal to any that do not terminate 
      timely.</para>

    <para>To power down a FreeBSD machine on architectures and systems
      that support power management, simply use the command
      <command>shutdown -p now</command> to turn the power off
      immediately.  To just reboot a FreeBSD system, just use
      <command>shutdown -r now</command>.  You need to be
      <username>root</username> or a member of
      <groupname>operator</groupname> group to run &man.shutdown.8;.
      The &man.halt.8; and &man.reboot.8; commands can also be used,
      please refer to their manual pages and to &man.shutdown.8;'s one
      for more information.</para>

    <note>
      <para>Power management requires &man.acpi.4; support in the kernel
	or loaded as module for FreeBSD&nbsp;5.X and &man.apm.4;
	support for FreeBSD&nbsp;4.X.</para>
    </note>

  </sect1>
</chapter>

<!-- 
     Local Variables:
     mode: sgml
     sgml-declaration: "../chapter.decl"
     sgml-indent-data: t
     sgml-omittag: nil
     sgml-always-quote-attributes: t
     sgml-parent-document: ("../book.sgml" "part" "chapter")
     End:
-->

