.\" $FreeBSD$
.PS

I:	box rad 0.10 wid 1 ht 0.55 "Internet" dashed;
	" (10.0.0.1/24) Default Router to Internet" at I.s below ljust;
	circle rad 0.02 fill 1 at I.s;
	line down at I.s;

A:	box "RouterA";
	" Interface xl0, 10.0.0.10/24" at A.n above ljust;
	" Interface xl1, 192.168.1.1/24" at A.s below ljust;
	" FreeBSD gateway" at A.e+(0.15,0) ljust;
	circle rad 0.02 fill 1 at A.n;
	circle rad 0.02 fill 1 at A.s;
	line down at A.s;
	
N1:	box ht .04 wid 2.8 fill with .nw at last line.end - (.4,0); 
	line at N1.se - (.4,0);


B:	box "RouterB";
	" 192.168.1.2/24" at B.n above ljust;
	" 192.168.2.1/24" at B.s below ljust;
	circle rad 0.02 fill 1 at B.n;
	circle rad 0.02 fill 1 at B.s;
	line;

N2:	box ht .04 wid 1.8 fill with .nw at last line.end - (.4,0);

N2a:	"Internal Net 2" at N2.s + (0,-.15);

N1a:	"Internal Net 1" at N1.sw + (.4,-.15);

.PE
